{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["PERFORMANCE SUMMARY"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PERFORMANCE SUMMARY","index":0,"n_rows":118,"n_cols":7,"rows_kept":118,"cut":false,"hidden":false,"merged":[[37,1,37,2],[10,1,10,3],[16,6,17,7],[64,1,65,5],[71,2,71,3],[75,1,76,1],[70,1,70,5],[66,1,66,5],[67,2,67,5],[68,2,68,5],[69,2,69,5],[60,1,60,2],[58,1,58,2],[59,1,59,2],[46,1,46,2],[19,6,35,6],[39,6,46,6],[63,3,63,4],[117,1,117,5],[48,1,48,2],[56,1,56,2],[39,3,45,3],[72,1,74,5],[91,1,91,2],[92,1,92,2],[96,1,96,5],[93,1,95,5],[87,1,87,2],[88,1,88,2],[88,4,88,5],[0,1,6,5],[11,1,11,3],[99,1,116,5],[98,1,98,5],[97,1,97,5],[12,1,12,3],[13,1,13,3],[15,1,15,2],[16,1,16,2],[7,1,7,5],[89,1,89,2],[90,1,90,2],[86,1,86,3],[86,4,86,5],[87,4,87,5],[38,1,38,2]]}
[null,"NBC(AE) 2023\nPERFORMANCE PATH \nSUMMARY APPLICATION "]
[]
[]
[]
[]
[]
[]
[null,"Section 1: Energy Model Summary"]
[]
[null,"Performance Path ",null," 9.36.5","9.36.7","EnerGuide v15"]
[null,"Project Address: ",null,null,"Zone 7A   HDD: ",5120]
[null,"Builder:",null,null,"Job Number:"]
[null,"BUILDING TYPE:",null,null,"DESIGN TYPE:"]
[null,"Building total area all floors including basement (m²)= ",null,null,"Orientation:"]
[null,null,null,"REFERENCE             "," PROPOSED "]
[null,"Airtightness ",null,"2.5 ACH@50Pa"]
[null,"Submit Blower Door Test Report? ",null,"N/A",null,"Provide for EnerGuide compliance path or if required for building code compliance "]
[]
[null,null,null,"REFERENCE  ETR          "," PROPOSED ETR","PROPOSED ASSEMBLY incl. insulation R-value"]
[null,"ROOF","Ceiling below attic",10.43,null,null,"PROPOSED ASSEMBLY (Primary thermal layer) including insulation R-value is to be indicated in the spaces for the applicable assemblies.  \n\nExamples are as follows: \n\n- Wall: 2x6@24\" oc / R22 batt ; \n- Roof truss: 24\" oc 2x4 bottom-chord / R57 (16\" cellulose loose-fill);\n- 2x4@16\" oc / R14 batt / 1.5\"EPS, \n- I joist 19.2\" oc/ 5\" 2lb sprayfoam R26 \n"]
[null,null,"Vault/flat roof",5.0199999999999996]
[null,"ABOVE-GROUND WALLS","Exterior walls",3.08]
[null,null,"Tall walls",3.08]
[null,null,"House to garage",3.08]
[null,null,"Other:",3.08]
[null,null,"Other:",3.08]
[null,null,"Other:",3.08]
[null,"RIM JOISTS All levels","Parallel (pony wall)",3.08]
[null,null,"Perpendicular",3.08]
[null,"ABOVE-GROUND FLOOR ","Cantilever/over exterior",5.0199999999999996]
[null,null,"Over garage",5.0199999999999996]
[null,"BELOW-GRADE WALLS ","Basement frostwall",3.46]
[null,null,"Basement walkout wall",3.46]
[null,"SLAB on GRADE ","Under, at edge & skirt",3.72]
[null,"BASEMENT FLOOR","Walkout-unheated floor",1.96]
[null,"FLOOR","Heated, in ground-contact",2.84]
[]
[null,"FDWR: see 9.36.5.14.(10)",null,null,null," "]
[null,"WINDOWS/DOORS  (U-value:  W/ (m² * K))  ",null,"U-value"," U-value"]
[null,null,"Picture    ",1.61,null,null,"1) Maximum U-value (“all windows to be of U-value ‘x’ or less” – model to use the U-value of ‘x’ in all windows as User Defined entry.  \nOR\n2) Individual U-values put on a window schedule.These individual U-values may come from either the manufacturer or from HOT2000 calculations. "]
[null,null,"Casement "]
[null,null,"Slider "]
[null,null,"Patio slider"]
[null,null,"Doors"]
[null,null,"Awning/hopper"]
[null,null,"Other"]
[null,"Solar Heat Gain Coefficient",null,0.26]
[]
[null,"Heat Recovery Ventilator proposed ?",null,"None"]
[null,"HRV Efficiency",null,"N/A"]
[null,"Space Heating Equipment Efficiency"]
[null,"Space Heating Equipment Efficiency"]
[null,"Ventilation Rate"]
[null,"Space Cooling Equipment Efficiency"]
[null,"Service Water Heater Efficiency"]
[null,"Service Water Heater Efficiency"]
[null,"Service Water recirculation pump included?"]
[]
[null,"HVAC (Heating, Cooling, Fan, Pump) (GJ)"]
[null,"Service Hot Water (GJ)"]
[null,"Total  annual energy consumption (GJ): ",null,{"$f":"SUM(D59:D60)","v":0},{"$f":"SUM(E59:E60)","v":0},{"$f":"1-E61/D61","v":{"$error":"#DIV/0!"}}]
[null,null,"Gross space heat loss",null,null,{"$f":"(D62-E62)/D62","v":{"$error":"#DIV/0!"}},"Gross space heat loss only required if following 9.36.7"]
[null,null,"Peak cooling load",null,null,{"$f":"IF(D63>E63,\"Fail, proposed peak must be lower than reference\",\"Pass\")","v":"Pass"},"Peak cooling load only required if following 9.36.7"]
[null,null,"Tier Achieved",{"$f":"IF(AND(F61>=0.7,F62>=0.4),\"5\",IF(AND(F61>=0.4,F62>=0.2),\"4\",IF(AND(F61>=0.2,F62>=0.1),\"3\",IF(AND(F61>=0.1,F62>=0.05),\"2\",1))))","v":{"$error":"#DIV/0!"}}]
[null,"Software Name/Version/Adaptations or workarounds:"]
[]
[null,"DECLARATION by person responsible for preparing the calculations used to demonstrate compliance with NBC(AE)2023 Division B Section 9.36.  Submit complete (proposed and reference) modelling report generated by ANSI/ASHRAE 140-compliant software to this Summary"]
[null,"Energy Advisor Firm:"]
[null,"Address:"]
[null,"Contact Email and Tel:"]
[]
[null,"Type Name to Sign:",null,null,"Date:"]
[null,"Section 2: Builder 9.36 Requirements"]
[]
[]
[]
[]
[null,null,null,null,"N","2.5 ACH@50Pa"]
[null,null,null,null,"NE","2.5 ACH@50Pa with Blower Door Test"]
[null,null,null,null,"E","< 2.5 ACH@50Pa with Blower Door Test"]
[null,null,null,null,"SE"]
[null,null,null,null,"S","Yes"]
[null,null,null,null,"SW","None"]
[null,null,null,null,"W"]
[null,null,null,null,"NW"]
[]
[null,"Primary Wall air barrier location/material:",null,null,"Ceiling below attic/vault/flat roof air barrier: "]
[null,"Interior poly with spray foam at rim joists and cantilevers            ",null,null,"Interior poly         "]
[null,"Interior poly with exterior flexible wrap at rim joists and cantilevers  ",null,null,"Other:      "]
[null,"Interior poly with sealants/tapes at floor, window, wall and ceiling intersections          "]
[null,"Exterior flexible air barrier system with all joints and edges sealed  "]
[null,"Exterior rigid air barrier system with all joints and edges sealed     "]
[null," Other: (specify)"]
[null,"Section 3: Builder Energy Data Disclosure"]
[]
[]
[null,"             By clicking this box you are agreeing to have this home and its EnerGuide label posted on the City of Edmonton's Change for Climate - EnerGuide for Homes Map. "]
[null,"You can view other participating builders and map here"]
[null,"Builder Specific Acknowledgement"]
[null,"If you agree, you confirm and warrant to the City that as of the date of your agreement to these Terms and the Privacy Policy, you were the owner of the property or properties provided to the City within the schedule (the “Schedule”). The City has the sole discretion to approve the form of Schedule and you confirm that the Schedule will be updated as required by the City. You acknowledge that it is your responsibility to provide the EnerGuide rating and associated documents to the new homeowner when you, as the Builder, transfer title to the new homeowner and also in accordance with the Natural Resources Canada's established processes. You also agree to inform the new homeowner that their EnerGuide rating has been shared via the City’s website. If the homeowner wishes, they can have the City remove their home EnerGuide rating from the site by contacting green.building@edmonton.ca.\n\nPlease carefully read the following, then click the approval box at the top of the section to confirm that you have read, understood, agree with the terms of the program.\n\nBy submitting this form, you confirm that:\n\nYou have read, understood and agree to the Terms and Privacy Policy. (http://ace.edmonton.ca/energuide/terms-and-privacy-policy)\nYou consent to personal information related to your participation in the Program being collected, used, stored, and disclosed in accordance with the Program’s Privacy Policy (see below).\nYou own (or owned) the properties in the “Schedule” at the time the EnerGuide label was issued.\nYou consent to Natural Resources Canada disclosing to the City the EnerGuide Home Evaluations.\nYou authorize the energy advisor or Service Organization who completed your EnerGuide Home Evaluations to provide copies of the EnerGuide labels for the properties in the Schedule.\nYou consent to the City of Edmonton collecting, using and storing the information provided to it by Natural Resources Canada, accessed through your provided EnerGuide file numbers, which may include personal information, related to your participation in the EnerGuide Rating Home Evaluations.\nYou consent to the City of Edmonton displaying the following on the City website:\nThe information provided by you (or your Service Organization) in Section B (Property Information),\nThe EnerGuide Information, including but not limited to parameters such as modeled energy consumption, heated floor area and modeled greenhouse gas emissions, and Copies of the EnerGuide labels produced as a result of the EnerGuide Home Evaluations.\nA photograph and address of the properties, displayed on a map.\nYou consent to the City of Edmonton sharing your information with its approved contractor for the purposes of administering and evaluating the program.\nYou consent to allow your EnerGuide rating, label and reports to remain on the City website until such time as the current titled owner of the property notifies the City via email at green.building@edmonton.ca with a request to remove the property from the City of Edmonton website."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"             By clicking this box you are opting out of having this home and its EnerGuide label posted on the City of Edmonton's Change for Climate - EnerGuide for Homes Map. "]